# 1. General Information

ESIM264 Configuration Tool is a software designed for operation with GSM Alarm and Control System ESIM264. Using this tool you will be able to quickly and easily set control parameters of the device, enter user data or simply change passwords which, otherwise, would have to be specified sending separately via SMS messages from your mobile phone.
This User guide provides detailed information about new functions and capabilities of the software as well as teaches how to configure ESIM264 security system.
Further you will see a brief description of every chapter:
2. Connection – a short instruction what the user must do every time before connecting ESIM264 device to the computer.
3. Control parameters – this chapter describes the procedure how the commands and functions described in section Settings(1), Settings(2) and iButton Keys should be properly used, i. e., you will be able to enter administrator telephone numbers, change the main password and other administration settings.
4. Zone settings – this chapter describes the procedure how the commands and functions described in section Zones should be properly used, i. e., you will be able to configurate the zone settings.
5. Output settings – this chapter describes the procedure how the commands and functions described in section PGM Outputs should be properly used, i. e., you will be able to configurate the output settings.
6. Monitoring Station settings - this section describes the procedure how the commands and functions described in section MS Settings should be properly used, i. e., you will be able to activate the mode when system is sending informational messages to monitoring stations via GSM audio channel or using GPRS connection.
7. Using wireless devices – this section describes the procedure how the commands and functions described in section RF Devices, Wireless Zones and Wireless Outputs should be properly used, i. e., you will be able to bind new wireless devices to the system, remove the old ones, configurate parameters and etc.
8. Automatic Output control – this section describes the procedure how the commands and functions described in section Control should be properly used, i. e., you will be able to specify that the system automatically activates certain outputs according to which event has started.